**Print Collection**

Blockout

Opak JET

Material: 82% PVC / 18% PES

Weight: 710 g/m2

**Features:**

High mechanical resistance

Opacity

Dimension stability

 Double side print

**Applications:**

Large format advertising for facades

 Signage (Double side print)

Banners (Double side print)

**Product attributes:**

Compatibility with Solvent, Eco-solvent, Uv and Latex Inks

FR certification available – B1, M2

Indoor and Outdoor

Up to 5 mters