**Terratex Collection**

Pollymesh 40 FR

180g/m2 polyester scrim with special resin coating, resulting on a PVC free mesh. Environmentally friendly and fire retardant.

Material: 53% PES / 47% RESIN

Weight: 180 g/m2

**Features:**

 PVC free

Light and easy to handle and instal

Crease resistant

Fire retardant

Recyclable under code nr. 1 (PET)

Good air permeability

**Applications:**

PVC free mesh applications

POS

Stands design and construction

Banners

Apllications requiring ecological approval

**Product attributes:**

Compatibility with Solvent, Eco-solvent, Uv and Latex Inks

FR certification available – B1

Indoor and Outdoor

Up to 5 meters