**X Collection**

Anti Curling

Print AC

330g/m2 PVC double coated polyester, with special textile structure for an anti-curling performance.

Material: 60% PVC / 40% PES

Weight: 330 g/m2

**Features:**

Brilliant colour reproduction

Anti-curling

Dimension Stable

Good flatness

**Applications:**

Roll up displays

Dysplay systems

Short/medium-term advertisements in Indoor or outdoor

**Product attributes:**

Compatibility with Solvent, Eco-solvent, Uv and Latex Inks

FR available – B1

Indoor e outdoor