**Walltex Collection**

Print N Tex

200g/m2 self-adhesive polyester fabric with special acrylate coating, which can be affixed to various types of surfaces. Environmentally friendly and fire retardant.

Material: 22% ACRYLATE / 78% PES

Weight: 200 g/m2

**Features:**

Quick application without special knowledge

Strong adhesion to various types of surfasse

Easily removable without leaving residues

Recyclable under code nr. 1 (PET)

No fraying

**Applications:**

Indoor Decoration

Store design

Wall coverings

Exhibitions

**Product attributes:**

Compatibility with Solvent, Eco-solvent, Uv and Latex Inks

FR available – B1

 Indoor