**Print Collection**

Frontlit

Print PA

Material: 71% PVC / 29% PES

Weight: 450 g/m2

**Features:**

High mechanical resistance

 Quick drying

 Easy to handle and instal

Weldable

**Applications:**

Banners

 Large format advertising

Displays POS

Posters

**Product attributes:**

Compatibility with Solvent, Eco-solvent, Uv and Latex Inks

FR certification available - B1, M1

Indoor and outdoor

Up to 5 meters