**X Collection**

Ceiling/ Wall

Soundtex 3.0

800g/m2 PVC coated polyester woven fabric, ideal for indoor wall decoration while allowing noise reduction

Material: 82% PVC / 18% PES

Weight: 800 g/m2

**Features:**

Sound absorbing

Dimension Stable

Good flatness

Up to 500cm

**Applications:**

Indoor Decoration

Store design

Mouse pads

Exhibitions

**Product attributes:**

Compatibility with Solvent, Eco-solvent, Uv and Latex Inks

Indoor