**Sublitex Collection**

Polyflag 110 FR

110g/m2 tearproof flag , 100% Polyester. Ideal for sublimation and UV. Environmentally friendly and fire retardant.

Material: 100% PES

Weight: 110 g/m2

**Features:**

Tearproof

Transparent

Heat set for sublimation

No fraying

Very good print through

**Applications:**

Indoor or Outdoor Flags

Banners

Flying type displays

**Product attributes:**

Transfer and direct dye sublimation

Compatibility with UV and Latex Inks

FR certification available – B1