**Print Collection**

Mesh

Print MS 55

Material: 67% PVC / 33% PES

Weight: 350 g/m2

**Features:**

 Easy to handle and instal

 High mechanical resistance

**Applications:**

Large format advertising for facades

Thermal protection

Signage

**Product attributes:**

Compatibility with Solvent, Eco-solvent, Uv and Latex Inks

FR certification available – B1, M1, NFPA-701

Outdoor

Up to 5 meters