**X Collection**

Roll up/ Display

Rolltex

370g/m2 PVC double coated polyester fabric, ideal for Roll up displays, distinguished by its texture and its similarity to the natural textile materials.

Material: 61% PVC / 39% PES

Weight: 370 g/m2

**Features:**

Brilliant colour reproduction

Dimension Stable

Good flatness

**Applications:**

Roll up displays

Dysplay systems

Short/medium-term advertisements in Indoor or outdoor

**Product attributes:**

Compatibility with Solvent, Eco-solvent, Uv and Latex Inks

FR certification available – B1

Indoor e outdoor