**Terratex Collection**

Terra Banner 200 FR

220g/m2 polyester banner with special resin coating, providing excellent whiteness and colorimetry. Environmentally friendly and fire retardant.

Material: 52% PES / 48% RESIN

Weight: 220 g/m2

**Features:**

PVC free

Light and easy to handle and instal

Crease resistant

Fire retardant

Recyclable under code nr. 1 (PET)

**Applications:**

Display frame systems

POS

Stands design and construction

Banners

Apllications requiring ecological approval

**Product attributes:**

Compatibility with Solvent, Eco-solvent, Uv and Latex Inks

 FR certification available – B1

 Indoor and Outdoor

Up to 5 meters