**Terratex Collection**

Terra light 200 FR

200g/m2 polypropylene coated polyester woven fabric for light boxes. Environmentally friendly and fire retardant.

Material: 17.5% PP

 82.5% PES

Weight: 200 g/m2

**Features:**

PVC Free

Light and easy to handle and instal

Crease resistant

Fire retardant

Recyclable under code nr. 1 (PET)

Textile looking

**Applications:**

Light boxes

Banners

Display frame systems

POS

Stands design and construction

Apllications requiring ecological approval

**Product attributes:**

Compatibility with Solvent, Eco-solvent, Uv and Latex Inks

 FR available – B1

 Indoor and Outdoor

Up to 5 meters