**Walltex Collection**

Print N Sub

210g/m2 self-adhesive polyester knitted fabric with special PU back coating, which can be affixed to various types of surfaces. Environmentally friendly and fire retardant

Material: 19% PU / 81% PES

Weight: 210 g/m2

**Features:**

Quick application without special knowledge

Strong adhesion to various types of surfasse

Easily removable without leaving residues

No fraying

**Applications:**

Indoor Decoration

Store design

Wall coverings

Exhibitions

**Product attributes:**

Transfer and direct dye sublimation

Compatibility with UV and Latex Inks

FR available – B1

Indoor