**Print Collection**

Mesh

Print MP 90 FR

Material: 58% PVC / 42% PES

Weight: 480 g/m2

**Features:**

 Double side print

 Good air permeabiliy

**Applications:**

Large format advertising for facades

 Signage (Double side)

**Product attributes:**

Compatibility with Solvent, Eco-solvent, Uv and Latex Inks

FR certification available – M2

Indoor and Outdoor

Up to 5 meters