**Sublitex Collection**

Terra Sub BW FR

270g/m2 resin coated polyester woven fabric, with black back, to give opacity and enhance your special applications. Environmentally friendly and fire retardant.

Material: 39% Resin/ 61% PES

Weight: 270 g/m2

**Features:**

Opacity

High quality colour reprodution

No fraying

Dimension stable

**Applications:**

Pop ups

Frames

Banners

Exhibitions

Rollups

**Product attributes:**

Transfer and direct dye sublimation

Compatibility with Uv and Latex Inks

FR available – B1

Indoor